Heights

Main ceiling: 95 in, 2.41 meters

Railing at highest: 8ft, 2.44m

Railing at lowest: 37in, 0.94

Cylinder bottom: 72in, 1.83

Railing width: .191

Indent for first thing: .305

mid cube 128 3.251

from rail to outer wall 44 1.118

Doors

Door: 80 in, 2.032 meters

Door frame: 2 in, .05 meters

Door inset from frame: .005

Door frame extruded: .01

Door width: 41.5in, 1.079

Handle from frame: 4in

Handle length 4.5in

Diameter 4in

Door window

47in from bottom: 1.19m

7x28in including frame: .18x.71

Frame: .04m

From side of the door: 6in, .15m

Frame out: .01m

Window inset from door: .01m

Slant to door window: .005m

Hallway width: 71.5in, 1.82m

Steps

Floor from top of railing: 44in, 1.18m

Step height: 7in, .18m (.1811)

Step width: 12in: .3m (.3011)

Front door

1-1/2 from side .04

1-3/4 from midline .04

2 for the lock .05

5-1/12 from top .14

5 from the side .13

10 from bottom .3

Front door

11 from top of window to top of door .28

2 from top of door .05

84 to top of door (so 82 for the door) 2.08

.75 out from door .02

2 out from window

38.5 handle from floor 1

Center room wall decoration

11 from first .28

24 from second .61

1.5 width .04

15to top .38

Indent .01

Inner door

Door side from front door frame: 5ft 8in

Door width 12ft6in

Main ceiling 13ft 7in

Corridor ceiling 7ft11in

Main entrance 42ft wide

Corridor length from office door 76ft 7/8in

Wall width

Corridor window .102

Middle Walls .165

Regular 5in .127

door frame sticks out 1/2in

Door frame: 6 in .152

Door 1 ¾ in thick .0444

41 ¾

34

Small door 2’4” wide

Stairs platform 60” wide 1.524